LAN3S-products-MIB DEFINITIONS ::= BEGIN

	    IMPORTS 
           enterprises, Counter, Gauge, IpAddress,
           NetworkAddress, TimeTicks
	           FROM RFC1155-SMI
            ifIndex, ipRouteDest, ipAdEntAddr, egpNeighAddr
	           FROM RFC1213-MIB
            atportIndex
               FROM RFC1243-MIB
            OBJECT-TYPE
               FROM RFC-1212;
DisplayString ::= OCTET STRING 

--OBJECT DEFINTIONS:  LAN3SBOKS  PRIVATE MIB
          --
          -- This MIB contains LAN3SBOKS product OIDs (used in sysObjectID)
          --

          LAN3SBOKS       OBJECT IDENTIFIER ::= { enterprises 10113 }

-- System Group  
	Lan3sSystem         OBJECT IDENTIFIER ::= { LAN3SBOKS  1 }
		Lan3sSysInfo	OBJECT IDENTIFIER ::= { Lan3sSystem 1 } 
			UnitName  	OBJECT-TYPE   
					SYNTAX	DisplayString
					ACCESS	read-only
					STATUS	mandatory
					DESCRIPTION	
		                " A printable ASCII string up to 32 octets long that is
		                 used to refer to a physical unit. This name is used
		                 in the prompt displayed at the maintenance terminal." 
					::= { Lan3sSysInfo 1 } 
			IdNumber		OBJECT-TYPE   
					SYNTAX	INTEGER
					ACCESS	read-write
					STATUS	mandatory
					DESCRIPTION	
		                " ID_Number" 
					::= { Lan3sSysInfo 2 } 
			SwVersion	OBJECT-TYPE   
					SYNTAX	DisplayString
					ACCESS	read-only
					STATUS	mandatory
					DESCRIPTION
		                   " A printable ASCII string representing the software
		                     version number of the running code."
					::= { Lan3sSysInfo 3 }
			FPGAVersion	OBJECT-TYPE   
					SYNTAX	DisplayString
					ACCESS	read-only
					STATUS	mandatory
					DESCRIPTION
		                   " A printable ASCII string representing the software
		                     version number of the running code."
					::= { Lan3sSysInfo 4 }
			LDRVersion	OBJECT-TYPE   
					SYNTAX	DisplayString
					ACCESS	read-only
					STATUS	mandatory
					DESCRIPTION
		                   " A printable ASCII string representing the software
		                     version number of the running code."
					::= { Lan3sSysInfo 5 }
			TrackVersion	OBJECT-TYPE   
					SYNTAX	DisplayString
					ACCESS	read-only
					STATUS	mandatory
					DESCRIPTION
		                   " A printable ASCII string representing the software
		                     version number of the running code."
					::= { Lan3sSysInfo 6 }
			  IAPVersion	OBJECT-TYPE   
					SYNTAX	DisplayString
					ACCESS	read-only
					STATUS	mandatory
					DESCRIPTION
		                   " A printable ASCII string representing the software
		                     version number of the running code."
					::= { Lan3sSysInfo 7 }
			  Reset		OBJECT-TYPE   
					SYNTAX	INTEGER {
						Reset (1)
					}
					ACCESS	read-write
					STATUS	mandatory
					DESCRIPTION
		                 " A Set  command on this object will cause an immediate reset
				   of the unit."
					::= { Lan3sSysInfo 8  }

		Lan3sRx	OBJECT IDENTIFIER ::= { Lan3sSystem 2 }
			CurrentLPD	OBJECT-TYPE  
					SYNTAX	INTEGER	{
						NoData (-1)
					}					
					ACCESS	read-only
					STATUS	deprecated
					DESCRIPTION
		                   " A printable ASCII string representing the Current L Photo Diode"
					::= { Lan3sRx 1 }
			ShadowCurrentLPD	OBJECT-TYPE   
					SYNTAX	INTEGER	{
						NoData (-1)
					}
					ACCESS	read-write
					STATUS	deprecated
					DESCRIPTION		
					"A printable ASCII string representing the SHADOW LEVEL OF RECEPTION"
					::= { Lan3sRx 2 }
			MaxCurrentLPD	OBJECT-TYPE   
					SYNTAX	INTEGER	{
						NoData (-1)
					}
					ACCESS	read-write
					STATUS	deprecated
					DESCRIPTION		
					"A printable ASCII string representing the MAX LEVEL OF RECEPTION"
					::= { Lan3sRx 3 }
			OverloadCurrentLPD	OBJECT-TYPE   
					SYNTAX	INTEGER	{
						NoData (-1)
					}
					ACCESS	read-write
					STATUS	deprecated
					DESCRIPTION		
					"A printable ASCII string representing the Current of an overload"
					::= { Lan3sRx 4 }
			UHI_Level 	OBJECT-TYPE
					SYNTAX	INTEGER	{
						NoData (-1)
					}
					ACCESS	read-write
					STATUS	deprecated
					DESCRIPTION
		            "A printable ASCII string representing the Set Uhi level."
					::= { Lan3sRx 5  }
			Voltage_LPD  OBJECT-TYPE   
					SYNTAX	INTEGER	{
						NoData (-1)
					}
					ACCESS	read-only
					STATUS	deprecated
					DESCRIPTION		
					"Voltage_LPD"
					::= { Lan3sRx 6 }
			Termal_LPD	OBJECT-TYPE   
					SYNTAX	INTEGER	{
						NoData (-1)
					}
					ACCESS	read-only
					STATUS	deprecated
					DESCRIPTION		
					"Termal_LPD K"
					::= { Lan3sRx 7 }
			ReceptionLevel	OBJECT-TYPE   
					SYNTAX	INTEGER	{
						NoData (-1)
					}
					ACCESS	read-only
					STATUS	deprecated
					DESCRIPTION		
					"ReceptionLevel"
					::= { Lan3sRx 8 }
			SaveRx 	OBJECT-TYPE
					SYNTAX	INTEGER	
						{ Save (1) }
					ACCESS	read-write
					STATUS	deprecated
					DESCRIPTION
		                 " Save Rx Data"
					::= { Lan3sRx 9  }
		Lan3sTx	OBJECT IDENTIFIER ::= { Lan3sSystem 3 }
		txNumber 	OBJECT-TYPE
				SYNTAX	INTEGER
				ACCESS	read-only
				STATUS	deprecated
				DESCRIPTION
		            " Number Tx"
				::= { Lan3sTx 1  }
		txTable OBJECT-TYPE 
			SYNTAX SEQUENCE OF TxEntry 
			ACCESS not-accessible 
			STATUS mandatory 
			DESCRIPTION "A list of transmiter entries. T
			he number of entries is given by the value of txNumber." 
					::= { Lan3sTx 2 }
		txEntry OBJECT-TYPE 
			SYNTAX TxEntry 
			ACCESS not-accessible 
			STATUS mandatory 
			DESCRIPTION "An interface entry containing objects at the 
				subnetwork layer and below for a particular transmiter." 
			INDEX { txIndex } 
				::= { txTable 1 } 
		TxEntry ::= 
			SEQUENCE {
				txIndex
					INTEGER,
				txBasic
					INTEGER,
				txBiasCurrent
					INTEGER,
				txModCurrent
					INTEGER,
				txDispCurrent
					INTEGER,			
				txCurrentLevel_0
					INTEGER,
				txCurrentLevel_100
					INTEGER,
				txLevelRadiation
			   		INTEGER,
				txTermal1
					INTEGER,
				txTermal2
					INTEGER,
				txSuppTeprm
					INTEGER,
				txSaveTx
					INTEGER
              }
			txIndex 	OBJECT-TYPE
					SYNTAX	INTEGER
					ACCESS	read-write
					STATUS	deprecated
					DESCRIPTION
		                 " Index Tx"
					::= { txEntry 1 }
			txBasic		OBJECT-TYPE
					SYNTAX	INTEGER {
						Basic (1),
						Second (2)
					}
					ACCESS	read-write
					STATUS	deprecated
					DESCRIPTION
		                 " 1-Basic"
					::= { txEntry 2  }
			txBiasCurrent	OBJECT-TYPE   
					SYNTAX	INTEGER	{
						NoData (-1)
					}
					ACCESS	read-write
					STATUS	deprecated
					DESCRIPTION		
					"A printable ASCII string representing the BiasCurrent"
					::= { txEntry 3 }
			txModCurrent	OBJECT-TYPE   
					SYNTAX	INTEGER	{
						NoData (-1)
					}
					ACCESS	read-write
					STATUS	deprecated
					DESCRIPTION		
					"A printable ASCII string representing the ModCurrent"
					::= { txEntry 4 }
			txDispCurrent	 OBJECT-TYPE   
					SYNTAX	INTEGER	{
						NoData (-1)
					}
					ACCESS	read-write
					STATUS	deprecated
					DESCRIPTION		
					"A printable ASCII string representing the Current of displacement"
					::= { txEntry 5 }
			txCurrentLevel_0	 OBJECT-TYPE   
					SYNTAX	INTEGER	{
						NoData (-1)
					}
					ACCESS	read-write
					STATUS	deprecated
					DESCRIPTION		
					"A printable ASCII string representing the Current of a level of 0 %"
					::= { txEntry 6 }
			txCurrentLevel_100	 OBJECT-TYPE   
					SYNTAX	INTEGER	{
						NoData (-1)
					}					
					ACCESS	read-write
					STATUS	deprecated
					DESCRIPTION		
					"A printable ASCII string representing the Current of a level of 100 %"
					::= { txEntry 7 }
			txLevelRadiation		OBJECT-TYPE   
					SYNTAX	INTEGER	{
						NoData (-1)
					}
					ACCESS	read-only
					STATUS	deprecated
					DESCRIPTION		
					"Level of radiation in %"
					::= { txEntry 8 }					
			txTermal1	 OBJECT-TYPE   
					SYNTAX	INTEGER	{
						NoData (-1)
					}
					ACCESS	read-only
					STATUS	deprecated
					DESCRIPTION		
					"txTermal1 K"
					::= { txEntry 9 }
			txTermal2	 OBJECT-TYPE   
					SYNTAX	INTEGER	{
						NoData (-1)
					}
					ACCESS	read-only
					STATUS	deprecated
					DESCRIPTION		
					"txTermal2 K"
					::= { txEntry 10 }
			txSuppTeprm	 OBJECT-TYPE   
					SYNTAX	INTEGER	{
						NoData (-1)
					}
					ACCESS	read-only
					STATUS	deprecated
					DESCRIPTION		
					"A printable ASCII string representing the supported temperature"
					::= { txEntry 11 }
			txSaveTx		OBJECT-TYPE
					SYNTAX	INTEGER	
					{	Save (1)}					
					ACCESS	read-write
					STATUS	deprecated
					DESCRIPTION
					"Save Tx Data"
					::= { txEntry 12  }
		Lan3sSystemData	OBJECT IDENTIFIER ::= { Lan3sSystem 4 }	
		AverAvailability	OBJECT-TYPE
					SYNTAX	DisplayString
					ACCESS	read-only
					STATUS	mandatory
					DESCRIPTION		
					"A printable ASCII string representing the Average availability"
					::= { Lan3sSystemData 1  }
		AverSpeed		OBJECT-TYPE
					SYNTAX	DisplayString
					ACCESS	read-only
					STATUS	mandatory
					DESCRIPTION		
					"A printable ASCII string representing the Average Speed"
					::= { Lan3sSystemData 2  }
		Distatance		OBJECT-TYPE
					SYNTAX	INTEGER {
						N/A (-70000)
					}
					ACCESS	read-only
					STATUS	mandatory
					DESCRIPTION		
					"Distatance"
					::= { Lan3sSystemData 3 }
		FsoSpeed		OBJECT-TYPE
					SYNTAX	INTEGER{
						S10(10),
						S100(100),
						S1000(1000)						
					}
					ACCESS	read-write
					STATUS	mandatory
					DESCRIPTION
					"Speed"
					::= { Lan3sSystemData 4  }
		Mode			OBJECT-TYPE
					SYNTAX	INTEGER {
						Auto (1),
						Manual (2),
						Scan (3)
					}
					ACCESS	read-write
					STATUS	mandatory
					DESCRIPTION
					"Mode 2-Manual 1 - Auto"
					::= { Lan3sSystemData 5  }
		LinkPortTP		OBJECT-TYPE
					SYNTAX	INTEGER {
						up (1),
						down (2),
					}
					ACCESS	read-only
					STATUS	mandatory
					DESCRIPTION		
					"A printable ASCII string representing the LinkPortTP"
					::= { Lan3sSystemData 6}
		SpeedPortTp 	OBJECT-TYPE
					SYNTAX	INTEGER {
						No (1)
						speed10 (10),
						speed100 (100),
						speed1000 (1000)
					}
					ACCESS	read-only
					STATUS	mandatory
					DESCRIPTION		
					"A printable ASCII string representing the LinkPortTP"
					::= { Lan3sSystemData 7}
		DuplexPortTp		OBJECT-TYPE
					SYNTAX	INTEGER {
						FD (1),
						HD (2)
					}
					ACCESS	read-only
					STATUS	mandatory
					DESCRIPTION		
					"A printable ASCII string representing the LinkPortTP"
					::= { Lan3sSystemData 8}
		InErrorsTp		OBJECT-TYPE
					SYNTAX	INTEGER
					ACCESS	read-only
					STATUS	mandatory
					DESCRIPTION
					"A printable ASCII string representing the InErrorsTp"
					::= { Lan3sSystemData 9  }
		SyncFsoPort		OBJECT-TYPE
					SYNTAX	INTEGER {
						Yes (1),
						No (2),
						LPBK_yes (3),
						LPBK_No (4)
					}
					ACCESS	read-only
					STATUS	mandatory
					DESCRIPTION
					"SyncFso 1-(Yes) 2 - (No)"
					::= { Lan3sSystemData 10  }
		FsoCorrections	OBJECT-TYPE
					SYNTAX	INTEGER
					ACCESS	read-only
					STATUS	mandatory
					DESCRIPTION
					"FsoCorrections"
					::= { Lan3sSystemData 11  }
		FsoErrors		OBJECT-TYPE
					SYNTAX	INTEGER
					ACCESS	read-only
					STATUS	mandatory
					DESCRIPTION
					"FsoErrors"
					::= { Lan3sSystemData 12 }
		StatCorrections OBJECT-TYPE
					SYNTAX	INTEGER
					ACCESS	read-only
					STATUS	mandatory
					DESCRIPTION
					"StatCorrections"
					::= { Lan3sSystemData 13 }
		StatErrors 		OBJECT-TYPE
					SYNTAX	INTEGER
					ACCESS	read-only
					STATUS	mandatory
					DESCRIPTION
					"StatErrors"
					::= { Lan3sSystemData 14 }
		StatErrSec		OBJECT-TYPE
					SYNTAX	INTEGER
					ACCESS	read-only
					STATUS	mandatory
					DESCRIPTION
					"	StatErrSec"
					::= { Lan3sSystemData 15 }
		ChangeSpeed		OBJECT-TYPE
					SYNTAX	INTEGER
					ACCESS	read-only
					STATUS	mandatory
					DESCRIPTION
					"	Change of speed"
					::= { Lan3sSystemData 16 }
		FsoPort		OBJECT-TYPE
					SYNTAX	INTEGER {
						Off (1),
						On (2)
					}
					ACCESS	read-only
					STATUS	mandatory
					DESCRIPTION
					"FsoPort"
					::= { Lan3sSystemData 17  }
		SysUpTime	OBJECT-TYPE 
					SYNTAX	TimeTicks
		       		ACCESS	read-only
		       		STATUS	deprecated
		       		DESCRIPTION
		      		"An object that contains the value of sysUpTime at
		      		the time that the value of the deprRptrGroupOperStatus
		      		object for this group last changed."
					::= { Lan3sSystemData 18 }
		SysTime		OBJECT-TYPE   
					SYNTAX	DisplayString
					ACCESS	read-write
					STATUS	mandatory
					DESCRIPTION
                 " The octet string of six bytes representing the
				 	time has the following format:
                  HH:MM:SS
                  where the valid range of values for each of the bytes
                  is as follows: HH (0..23):MM (0..59): SS (0..59)"
					::= { Lan3sSystemData 19 }
		SysDate	  OBJECT-TYPE   
					SYNTAX	DisplayString
					ACCESS	read-write
					STATUS	mandatory
					DESCRIPTION
                 " The octet string of six bytes representing the 
				 	date has the following format:
                  YY/MM/DD
                  where the valid range of values for each of the bytes
                  is as follows: YY (0..65535)/MM (1..12))DD(1..31)"
					::= { Lan3sSystemData 20 }
		SwiTermal   OBJECT-TYPE
					SYNTAX	INTEGER	{
						NoData (0)
					}
					ACCESS	read-only
					STATUS	mandatory
					DESCRIPTION
					"SwiTermal K"
					::= { Lan3sSystemData 21 } 
		ClrStatCnt		OBJECT-TYPE
					SYNTAX	INTEGER {
						Clr (1)
					}
					ACCESS	read-write
					STATUS	mandatory
					DESCRIPTION
					"ClrStatCnt"
					::= { Lan3sSystemData 22 }
		StatQulity	OBJECT-TYPE
					SYNTAX	INTEGER 
					ACCESS	read-only
					STATUS	mandatory
					DESCRIPTION
					"StatQulity"
					::= { Lan3sSystemData 23 }
		MediaCtrl	OBJECT-TYPE
					SYNTAX	INTEGER {
						AUX (0),
						FSO (1),
						OFF (2),
						AUTO (3),
						TRUNK (4),
					}
					ACCESS	read-write
					STATUS	mandatory
					DESCRIPTION
					"ClrStatCnt"
					::= { Lan3sSystemData 24 }					
		Lan3sMon	OBJECT IDENTIFIER ::= { Lan3sSystem 5 }
		monNumber 	OBJECT-TYPE
				SYNTAX	INTEGER
				ACCESS	read-only
				STATUS	deprecated
				DESCRIPTION
		            " Number Device"
				::= { Lan3sMon 1  }
		monTable OBJECT-TYPE 
			SYNTAX SEQUENCE OF MonEntry 
			ACCESS not-accessible 
			STATUS mandatory 
			DESCRIPTION "" 
					::= { Lan3sMon 2 }
		monEntry OBJECT-TYPE 
			SYNTAX MonEntry 
			ACCESS not-accessible 
			STATUS mandatory 
			DESCRIPTION "" 
			INDEX { monIndex } 
			::= { monTable 1 } 
		MonEntry ::= 
			SEQUENCE {
				monIndex
					INTEGER,
				monDescr
					DisplayString,
				monIdNum
					INTEGER,
				monSpeed
					INTEGER,
				monMode
					INTEGER,			
				monTpLink
					INTEGER,
				monSpeedPortTp
					INTEGER,
				monTpDuplex
					INTEGER,
				monFsoPort
			   		INTEGER,
				monSyncFsoPort
					INTEGER,
				monFsoErrors
					INTEGER,
				monFsoCorrections
					INTEGER,
				monSysUpTime
					INTEGER,
				monStatErrors
					INTEGER,
				monStatCorrections
					INTEGER,
				monStatErrSec
					INTEGER,
				monChangeSpeed
					INTEGER,
				monReceptionLevel
					INTEGER,
				monUHI_Level
					INTEGER,
				monTermal_LPD
					INTEGER,
				monModeTx_0
					INTEGER,
				monModeTx_1
					INTEGER,
				monRxQuality
					INTEGER,
				monAUXStatus
					INTEGER,
				monChangeAux
					INTEGER, 
				monMediaType
					INTEGER
			}

			monIndex 	OBJECT-TYPE
					SYNTAX	INTEGER
					ACCESS	read-write
					STATUS	deprecated
					DESCRIPTION
		                 " Index Device"
					::= { monEntry 1 }
			monDescr	OBJECT-TYPE   
					SYNTAX	DisplayString
					ACCESS	read-only
					STATUS	deprecated
					DESCRIPTION
		                   " A printable ASCII string "
					::= { monEntry 2 }
			monIdNum	OBJECT-TYPE   
					SYNTAX	INTEGER{
					NoData (-1)
					}
					ACCESS	read-only
					STATUS	deprecated
					DESCRIPTION		
					"Id number"
					::= { monEntry 3 }
			monSpeed	OBJECT-TYPE
					SYNTAX	INTEGER{
						S10(10),
						S100(100),
						S1000(1000),
						NoData (-1)						
					}
					ACCESS	read-only
					STATUS	deprecated
					DESCRIPTION
					"Speed"
					::= { monEntry 4 }
			monMode		OBJECT-TYPE
					SYNTAX	INTEGER {
						Auto (1),
						Manual (2),
						Scan (3),
						NoData (-1)
					}
					ACCESS	read-only
					STATUS	deprecated
					DESCRIPTION
					"Mode 2-Manual 1 - Auto"
					::= { monEntry 5 }
			monTpLink	OBJECT-TYPE
					SYNTAX	INTEGER {
						up (1),
						down (2),
						NoData (-1)
					}
					ACCESS	read-only
					STATUS	deprecated
					DESCRIPTION		
					"LinkPortTP"
					::= { monEntry 6 }
			monSpeedPortTp 	OBJECT-TYPE
					SYNTAX	INTEGER {
						No (1),
						speed10 (10),
						speed100 (100),
						speed1000 (1000),
						NoData (-1)
					}
					ACCESS	read-only
					STATUS	deprecated
					DESCRIPTION		
					"A printable ASCII string representing the LinkPortTP"
					::= { monEntry 7 }
			monTpDuplex	OBJECT-TYPE
					SYNTAX	INTEGER {
						FD (1),
						HD (2),
						NoData (-1)
					}
					ACCESS	read-only
					STATUS	deprecated
					DESCRIPTION		
					"Duplex Tp Port"
					::= { monEntry 8 }
			monFsoPort	OBJECT-TYPE
					SYNTAX	INTEGER {
						Off (1),
						On (2),
						NoData (-1)
					}
					ACCESS	read-only
					STATUS	deprecated
					DESCRIPTION
					"FsoPort"
					::= { monEntry 9 }					
			monSyncFsoPort		OBJECT-TYPE
					SYNTAX	INTEGER {
						Yes (1),
						No (2),
						LPBK (3),
						NoData (-1)
					}
					ACCESS	read-only
					STATUS	deprecated
					DESCRIPTION
					"SyncFso 1-(Yes) 2 - (No)"
					::= { monEntry 10 }			
			monFsoErrors		OBJECT-TYPE
					SYNTAX	INTEGER {
						NoData (-1)
					}
					ACCESS	read-only
					STATUS	deprecated
					DESCRIPTION
					"FsoErrors"
					::= { monEntry 11 }
			monFsoCorrections	OBJECT-TYPE
					SYNTAX	INTEGER {
						NoData (-1)
					}
					ACCESS	read-only
					STATUS	deprecated
					DESCRIPTION
					"FsoCorrections"
					::= { monEntry 12 }
			monSysUpTime	OBJECT-TYPE 
					SYNTAX	TimeTicks
					ACCESS	read-only
					STATUS	deprecated
					DESCRIPTION
					"	SysUpTime"
					::= { monEntry 13 }
			monStatErrors 		OBJECT-TYPE
					SYNTAX	INTEGER {
						NoData (-1)
					}
					ACCESS	read-only
					STATUS	deprecated
					DESCRIPTION
					"StatErrors"
					::= { monEntry 14 }
			monStatCorrections	OBJECT-TYPE
					SYNTAX	INTEGER {
						NoData (-1)
					}
					ACCESS	read-only
					STATUS	deprecated
					DESCRIPTION
					"StatCorrections"
					::= { monEntry 15 }		
			monStatErrSec		OBJECT-TYPE
					SYNTAX	INTEGER {
						NoData (-1)
					}
					ACCESS	read-only
					STATUS	deprecated
					DESCRIPTION
					"	StatErrSec"
					::= { monEntry 16 }
			monChangeSpeed		OBJECT-TYPE
					SYNTAX	INTEGER {
						NoData (-1)
					}
					ACCESS	read-only
					STATUS	deprecated
					DESCRIPTION
					"	Change of speed"
					::= { monEntry 17 }
			monReceptionLevel	OBJECT-TYPE   
					SYNTAX	INTEGER {
						NoData (-1)
					}
					ACCESS	read-only
					STATUS	deprecated
					DESCRIPTION		
					"ReceptionLevel"
					::= { monEntry 18 }
			monUHI_Level 	OBJECT-TYPE
					SYNTAX	INTEGER {
						NoData (-1)
					}
					ACCESS	read-only
					STATUS	deprecated
					DESCRIPTION
		            		"Uhi level."
					::= { monEntry 19 }
			monTermal_LPD	OBJECT-TYPE   
					SYNTAX	INTEGER	{
						NoData (0)
					}
					ACCESS	read-only
					STATUS	deprecated
					DESCRIPTION		
					"Termal_LPD K"
					::= { monEntry 20 }
			monModeTx_0	OBJECT-TYPE   
					SYNTAX	INTEGER{
						N/A (0),
						On (1),
						Off (2),
						NoData (-1)
					}
					ACCESS	read-only
					STATUS	deprecated
					DESCRIPTION		
					"monModeTx_0"
					::= { monEntry 21 }
			monModeTx_1	OBJECT-TYPE   
					SYNTAX	INTEGER{
						N/A (0),
						On (1),
						Off (2),
						NoData (-1)
					}
					ACCESS	read-only
					STATUS	deprecated
					DESCRIPTION		
					"monModeTx_1"
					::= { monEntry 22 }
			monRxQuality	OBJECT-TYPE
					SYNTAX	INTEGER {
						NoData (-1)
					}
					ACCESS	read-only
					STATUS	deprecated
					DESCRIPTION
		            "RxQuality."
					::= { monEntry 23 }
			monAUXStatus	OBJECT-TYPE
					SYNTAX	INTEGER {
						N/A (0),
						On (1),
						Off (2),
						Ds (3),
						NoData (-1)
					}
					ACCESS	read-only
					STATUS	deprecated
					DESCRIPTION
		            "AUXStatus."
					::= { monEntry 24 }
			monChangeAux	OBJECT-TYPE
					SYNTAX	INTEGER {
						NoData (-1)
					}
					ACCESS	read-only
					STATUS	deprecated
					DESCRIPTION
					"Change of Aux"
					::= { monEntry 25 }
			monMediaType	OBJECT-TYPE
					SYNTAX	INTEGER {
						AUX (0),
						FSO (1),
						OFF (2),
						AUTO (3),
						TRUNK (4),
						NoData (-1)
					}
					ACCESS	read-only
					STATUS	deprecated
					DESCRIPTION
		            "AUXStatus."
					::= { monEntry 26 }

END          